**218e Charging Instructions**

**Connections**

1. SDC Connector on Accumulator
2. VBATT Connector on Accumulator
3. LVMS Connector on Accumulator
4. MISC Connector on Accumulator
5. Tape TSMP Connector
6. Connect HVD
7. AC Connector on Charger
8. DC Connector on Charger
9. Control Connector on Charger
10. J1772 Plug (EVSE) to charger
11. Plug EVSE into wall

**Startup**

1. With J1772 and Charger LV power unplugged, turn on the LV supply
2. Wait 15 seconds
3. Plug in the J1772 connector and Charger LV Power
4. Open the Shutdown Button
5. Flip set/reset switch
6. Listen for contactors to close, and check the AIR status in the AuxMCU Flags Message
7. Send the Charger Command Message From CANoe at 16 Amps and 249.6 Volts

